#### Five Minute Settlements Project: High-Level Impact Assessment

|  |  |  |  |
| --- | --- | --- | --- |
| Document Title | Service Level Procedure – Metering Data Provision Services | | |
| Rule Consultation Req. | Yes | Priority | High |
| Prepared by |  | Business Owner | Metering |
| Consultation Group | Metering | Consultation Package |  |
| Link | [SLP - MDP](http://www.aemo.com.au/-/media/Files/Electricity/NEM/Retail_and_Metering/Metering-Procedures/2017/SLP-MDP-Services.pdf) | | |

|  |  |  |  |
| --- | --- | --- | --- |
| Description of Document | The SLP – MDP details the obligations, technical requirements, measurement processes and performance requirements to be met by MDPs in the provision of metering data services for all metering installations types and the maintenance of a metering data services database | | |
| Precedent Procedures / External Documents | Metrology Procedure Part B  MSATS, MDM and NMI Procedures | Dependent Procedures / External Documents | MDFF Specification |
| Summary of Changes – Five Minute Settlements | Remove meter churn scenario – type 6 replaced with new type 6  Include provisions to support MDFF metering data delivery to AEMO | | |
| Summary of Potential Changes – Global Settlements | Remove references as required concerning: Local Retailer, 1st Tier and 2nd Tier  Update required regarding cross boundary/border supply points between distribution networks or Local Retailer regions  Review data stream activation requirements for type 6 meters that were tier 1 | | |
| External Stakeholder Impacted | Yes | AEMO Business Units Impacted | Settlements  Prudentials |
| Issues for Stakeholder Consultation | Metering Data Processing Requirements – current requirement to aggregate into 30-minute interval net Datastream prior to delivery to AEMO  Method of Delivery of Data – current requirement for MDM data file | | |
| System Impact | Yes | | |